OptiPlex 3010 Mini Tower

|  |  |
| --- | --- |
| **Part** | **Name** |
| **PROCESSOR** | Intel® Pentium® Processor G645 (3M Cache, 2.90 GHz, w/HD Graphics) |
| **OPERATING SYSTEM** | Windows 7 Home Premium, No Media, 32-bit, English |
| **OFFICE SOFTWARE** | Microsoft® Office Trial |
| **MEMORY** | 2GB, NON-ECC, 1600MHZ DDR3,1DIMM |
| **OPTICAL DRIVE** | 16X DVD-ROM SATA, Data Only |
| **HARD DRIVE** | 250GB 3.5" SATA 3.0Gb/s and 8MB DataBurst Cache™ |
| **GRAPHICS** | Intel® Integrated Graphics w/Single HDMI/VGA |
| **SUPPORT PLAN** | 3 Year Basic Hardware Service with 3 Year NBD Limited Onsite Service After Remote Diagnosis |
| **KEYBOARD** | Dell KB212-B USB 104 Quiet Key Keyboard,English |
| **SECURITY SOFTWARE** | Trend Micro Worry-Free Business Security Services, 30-days |
| **BASE/ POWER SUPPLY** | OptiPlex 3010 Minitower for Standard Power Supply |
| **SPEAKERS** | Internal Dell Business Audio Speaker |
| **MOUSE** | Dell MS111 USB Optical Mouse |
| **POWER SUPPLY** | OptiPlex 3010 Minitower w/ Standard PSU |
| **THERMALS** | Heat Sink, Mainstream, Minitower |
| **SYSTEM DOCUMENTATION** | Documentation English and French |

Dell Professional P1913 19" Monitor with LED

|  |  |
| --- | --- |
| **Part** | **Name** |
| **Diagonally Viewable Size** | 48.26 cm  19 Inches (19-inch wide viewable image size) |
| **Aspect Ratio** | Widescreen (16:10) |
| **Panel Type** | TN (Twisted Nematic), anti glare with hard coat 3H |
| **Optimal resolution** | 1440 x 900 at 60 Hz |
| **Contrast Ratio** | 1000: 1 (typical)  2 Million:1 (Max) (Dynamic Contrast Ratio) |
| **Brightness** | 250 cd/m2 (typical) |
| **Response Time** | 5 ms (back to white) |
| **Max Viewing Angle** | (160° vertical / 170° horizontal) |
| **Color Support** | 16.7 million colors |
| **Pixel Pitch** | 0.248 mm |
| **Panel Backlight** | LED |
| **Display Type** | Widescreen Flat Panel Display |
| **Connectivity** | 1 Digital Visual Interface connectors (DVI-D) with HDCP  1 Video Graphics Array (VGA)  1 DisplayPort (version 1.2)  1 USB 2.0 upstream port  2 USB 2.0 downstream ports)  DC power connector for Dell Soundbar (AX510 only) |

PowerEdge T320

|  |  |
| --- | --- |
| **Part** | **Name** |
| **Chassis Configuration** | Chassis with up to 8, 3.5" Hot-Plug Hard Drives and Embedded SATA |
| **Processor** | Intel® Xeon® E5-2420 1.90GHz, 15M Cache, 7.2GT/s QPI, Turbo, 6C, 95W, Max Mem 1333MHz |
| **Memory Configuration Type** | Performance Optimized |
| **Memory DIMM Type and Speed** | 1333 MHz UDIMMs |
| **Memory Capacity** | 4GB UDIMM, 1333 MT/s, Low Volt, Dual Rank, x8 Data Width |
| **Operating System** | Windows Server 2008 R2 SP1, Standard Edition,x64, Includes 5 CALS |
| **OS Media Kits** | Windows Server®2008SP2,Standard ED, x86/x64,Downgrade Media |
| **RAID Configuration** | SW RAID 5 for S110 (3-4 SATA/SATA SSD HDDs) |
| **RAID Controller** | Software RAID (for Microsoft OS Only) |
| **Hard Drives** | 500GB 7.2K RPM SATA 3Gbps 3.5in Hot-plug Hard Drive x3 |
| **Embedded Systems Management** | Basic Management |
| **Add-in Network Adapter** | On-Board Dual Gigabit Network Adapter |
| **Power Supply** | Single, Cabled Power Supply , 350W |
| **Power Cords** | NEMA 5-15P to C13 Wall Plug, 125 Volt, 15 AMP, 10 Feet (3m), Power Cord |
| **Power Management BIOS Settings** | Power Saving Dell Active Power Controller |
| **Rack Rails and Casters** | Tower Chassis, No Casters |
| **System Documentation** | Electronic System Documentation and OpenManage DVD Kit |
| **Server Accessories** | Keyboard and Optical Mouse, USB, Black, English, with 17 LCD Monitor |
| **Hardware Support Services** | 3Yr Basic Hardware Warranty Repair: 5x10 HW-Only, 5x10 NBD Onsite |

# NetGear Ultra 4 Network Attached Storage

|  |  |
| --- | --- |
| **Part** | **Name** |
| **Processor Brand** | Intel |
| **Processor Class** | Atom |
| **Processor Speed** | 1.66 GHz |
| **Dimensions** | 5.28 x 8.07 x 8.78 in |
| **Memory Type** | DDR2 |
| **Total Memory** | 1 GB |
| **USB Ports (Total)** | 3 |
| **RJ-45 Ports** | 2 |
| **Interface Type** | Gigabit Ethernet |
| **Data Transfer Rate** | 80 Mbps |
| **Compatible RAID Levels** | RAID 0, 1, 5 |
| **Number Of Hard Drives Bays** | 4 |

HP EliteBook 2570p Notebook PC

|  |  |
| --- | --- |
| **Part** | **Name** |
| **Operating system** | Windows 7 Professional 64bit |
| **Processor** | Intel® Core™ i3-3120M (2.50 GHz, 3 MB L3 cache, 2 cores) |
| **Chipset** | Mobile Intel® QM77 Express |
| **Environmental** | BFR/PVC-free |
| **Weight** | Starting at 3.6 lb (Starting at 1.63 kg) |
| **Dimensions (W x D x H)** | 12.02 x 8.23 x 1.08 in (30.5 x 20.9 x 2.7 cm) |
| **Memory, maximum** | 16 GB 1600 MHz DDR3 SDRAM |
| **Memory slots** | 2 SODIMM |
| **Internal drive** | SATA II (7200 rpm) 500 GB |
| **Optical drive** | DVD+/-RW SuperMulti DL; DVD-ROM |
| **Display** | 12.5" diagonal LED-backlit HD anti-glare (1366 x 768) |
| **Graphics** | Integrated Intel® HD Graphics 4000 |
| **Ports** | 1 USB 3.0 1 USB 2.0 charging 1 eSATA/USB 2.0 combo 1 combo stereo headphone/mic jack 1 AC power 1 RJ-11 1 RJ-45 1 docking connector 1 1394a 1 DisplayPort 1.1a 1 VGA |
| **Slots** | 1 Express Card/34 1 Secure Digital |
| **Audio** | SRS Premium Sound PRO; Integrated stereo speakers; Integrated dual-microphone array; Combo headphone/microphone jack |
| **Keyboard** | Spill-resistant keyboard and drain |
| **Input devices** | Touchpad with on/off button, two-way scroll, gestures, two pick buttons; Pointstick with two additional pointstick buttons |
| **Network interface** | Integrated Intel 82579LM Gigabit Network Connection (10/100/1000) |
| **Wireless** | Broadcom 802.11a/b/g/n HP Integrated Module with Bluetooth 4.0+ EDR |
| **Energy efficiency** | ENERGY STAR® qualified configurations available; EPEAT® where HP registers commercial desktop products. See www.epeat.net for registration status in your country. |
| **Power supply** | 65W Smart AC adapter; HP Fast Charge (not supported on 9-cell battery) |
| **Battery  type** | 6-cell (62 WHr) Li-Ion |
| **Battery life** | 6-cell (62 WHr) Li-Ion: Up to 9 hours and 15 minutes |
| **Security management** | Standard: HP Client Security (Windows 8 only) HP ProtectTools TPM Embedded Security Chip 1.2 Drive Encryption Smart Card Reader Credential Manager Password Manager One Step Logon Face Recognition SpareKey Device Access Manager w/ JITA Security lock slot Optional: Microsoft Defender (Windows 8 only, includes Microsoft Security Essentials) Microsoft Security Essentials HP Fingerprint Sensor HP Privacy Filter HP Combo Lock |

HP 2570p Docking Station

|  |  |
| --- | --- |
| **Part** | **Name** |
| **Ports** | 1 eSATA; 4 USB (3 USB 3.0, 1 USB 2.0 powered); 1 DisplayPort 1.2; 1 VGA; 2 Audio (Audio in, audio out (does not support mic out)); 1 LAN/Ethernet jack |
| **Power requirements** | Energy-efficient 65W Smart AC adapter |
| **Product dimensions (W x D x H)** | 14.1 x 4.8 x 2 in |
| **Security management** | HP Lock (Lock not included) |
| **Manufacturer Warranty** | HP Ultra-light Docking Stations are supported by a one-year limited warranty. Additional support is available 24 hours a day, seven days a week by phone as well as online support forums. NOTE: Certain restrictions and exclusions apply. Consult the HP Customer Support Center for details. |
| **Weight** | 2.04 lb / 0.93 kg |

TrippLite SMARTPRO® Series - SMART3000NET

|  |  |
| --- | --- |
| **Part** | **Name** |
| **Output Volt Amp Capacity (VA)** | 3000 |
| **Output kVA capacity (kVA)** | 3 |
| **Output Watt Capacity (watts)** | 2400 |
| **Output kW capacity** | 2.4 |
| **Output power factor** | 0.8 |
| **Nominal Output Voltage(s) Supported** | 120V |
| **Frequency compatibility** | 60 Hz |
| **Output voltage regulation (line mode)** | -13% / +5% |
| **Output voltage regulation (Battery mode)** | +/- 5% |
| **Built-in UPS output receptacles** | 4 5-15R outlet(s); 4 5-15/20R outlet(s) |
| **Built-in controllable switched load banks** | Three switchable single-outlet 5-15R load banks |
| **Output circuit breaker** | 15A branch rated (x2) - each breaker protects 4 outlets |
| **Output AC waveform (AC mode)** | Sine wave |
| **Output AC waveform (battery mode)** | PWM sine wave |
| **Rated input current (at maximum load)** | 22A |
| **Nominal Input Voltage(s) Supported** | 120V AC |
| **UPS input connection type** | L5-30P |
| **UPS Input cord length (ft.)** | 8 |
| **UPS Input cord length (m)** | 2.4 |
| **Recommended Electrical Service** | 30A 120V |
| **Input cord length (ft.)** | 8 |
| **Full load runtime (minutes)** | 7 min. (2400w) |
| **Half load runtime (minutes)** | 23 min. (1200w) |
| **Expandable battery runtime** | Extended runtime supported via optional external battery packs |
| **External battery pack compatibility** | BP24V28-2U (limit 1); BP24V70-3U (multi-pack compatible) |
| **DC system voltage (VDC)** | 24 |
| **Battery recharge rate (included batteries)** | Less than 9 hours from 10% to 90% |
| **Transfer time** | 2-4 milliseconds |
| **Low voltage transfer to battery power (setpoint)** | 87 |
| **High voltage transfer to battery power (setpoint)** | 140 |
| **Product Warranty Period (Worldwide)** | 2-year warranty, 3 year with [registration](http://www.tripplite.com/en/support/Product-Warranty-Step-1.cfm). Note: [registration](http://www.tripplite.com/en/support/Product-Warranty-Step-1.cfm) is required for 3-year warranty. |
| **Connected Equipment Insurance (U.S., Canada & Puerto Rico)** | $250,000 [Ultimate Lifetime Insurance](http://www.tripplite.com/en/support/insurance-coverage-and-claims.cfm) |

Xerox WorkCentre 6015

|  |  |
| --- | --- |
| **Part** | **Name** |
| **Standard functions** | Copy, Email, Fax, Print, Scan |
| **Print speed** | Color: up to 12 ppm Black: up to 15 ppm |
| **Connectivity** | 10/100BaseTX Ethernet, USB 2.0, Wi-Fi |
| **Document handler** | Automatic Document Feeder Capacity: 15 sheets |
| **Output capacity** | 100 sheets |
| **Two-sided output** | Manual |
| **Fax features** | Auto redial, Auto reduction, Delayed fax, Junk fax barrier, Last number redial, Memory receive, Polling\*  \* - Analog phone line required. |
| **Scan destinations** | Scan to USB, Scan to email, Scan to network |
| **Security features** | IPv6 |
| **Duty cycle** | Up to 30,000 images/month1 |
| **Recommended monthly print volume** | Up to 1,500 pages |
| **Warranty** | One-year Quick Exchange, Xerox Total Satisfaction Guarantee |

Printing

|  |  |
| --- | --- |
| **Part** | **Name** |
| **First-page-out time, printing** | As fast as 17 seconds color / 14 seconds black and white |
| **Maximum print resolution** | 1200 x 2400 dpi |
| **Processor** | 295 MHz |
| **Print memory (standard)** | 128 MB standard |
| **Page Description Languages (PDL)** | Host-based |
| **Print features** | Black and white only print mode, Built-in support links, Collation, Custom page size, Draft mode, Fit-to-page, N-up, Poster printing, Run Black, Scaling, Watermarks |

Terminals – Samsung Galaxy Tab 2 7.0

|  |  |
| --- | --- |
| **Part** | **Name** |
| Operation System | Android 4.0 (Ice Cream Sandwich) |
| Browser | Android 4.0 (Ice Cream Sandwich) |
| Display | 178mm (7") 1024 x 600 (WSVGA) PLS TFT LCD |
| Capacity | 8 GB Micro SD card slot supports up to 32GB |
| Processor | 1GHz Dual Core Processor |
|  |  |
| Camera Resolution | 3 Megapixel Rear Camera |
| Flash | N/A |
| Auto Focus | Yes |
| Shot mode | 3 Shot Modes available |
| Photo Effects | 3 Photo Effects available |
| White Balance | N/A |
|  |  |
| Video player | AVI, DIVX, FLV, MKV, MP4, WEBM, WMV |
| Video recording | Yes |
| Video Messaging | No |
| Input Device | Touch Input |
|  |  |
| Music Player | AAC, AAC+, AC-3, EAAC+, FLAC, MP3, OGG, WMA |
| Polyphonic Ringtones | Yes |
| MP3 Ringtone | Yes |
| DRM | DRM Available (OMA v1.0 FL) |
| 3D Sound Technology | N/A |
| Music Library | Yes |
|  |  |
| Email | Yes |
| SMS, EMS, MMS | SMS, MMS, Video messaging supported |
| T9 Predictive Text | Yes |
| vCard / vCalendar | No |
| Instant Messaging | Yes |
|  |  |
| Bluetooth | BT 3.0 |
| USB | 2.0 High Speed (USB 2.0 Host) |
| Internet HTML Browser | Yes |
| SyncML (DM) | Yes |
| WAP | N/A |
| AGPS | No |
| TV-Output | N/A |
|  |  |
| Battery | Yes, Rechargable via USB |
|  |  |
| Dimensions | 193 x 122 x 10.4mm |
| Weight | 344g |

**Specifications Not Available**

* Seagate 500gb HDD x 3
* Cisco Catalyst switch 3750